,_DistributedBy##OTHER##,_CurrentRevision##OTHER##,_CreatedBy##OTHER##,_BimSpecGuid##OTHER##,_BSBibleVersion##OTHER##,_Author##OTHER##,TMU_Width##LENGTH##MILLIMETERS,Water_Content##OTHER##,Water Regulations Compliant##OTHER##,WarrantyStartDate##OTHER##,WarrantyGuarantorParts##OTHER##,WarrantyDurationUnit##OTHER##,WarrantyDurationParts##OTHER##,WarrantyDescription##OTHER##,Voltage##ELECTRICAL_POTENTIAL##VOLTS,URL##OTHER##,Type##OTHER##,Supply_Phase##OTHER##,Standing_Heat_Loss##OTHER##,Shipping_Weight##OTHER##,Shape##OTHER##,SerialNumber##OTHER##,Safety_Valve_Connection_Type##OTHER##,Referenced_Standard##OTHER##,Product_Range##OTHER##,Product_Model_Number##OTHER##,Product_Literature##OTHER##,Overall_Width##LENGTH##MILLIMETERS,Overall_Length##LENGTH##MILLIMETERS,Overall_Height##LENGTH##MILLIMETERS,OutletHeatPump_Connection_Type##OTHER##,OutletHeatPump_Connection_Size##OTHER##,OutletHeatPump_Height##LENGTH##MILLIMETERS,OutletHC_Connection_Type##OTHER##,OutletHC_Connection_Size##OTHER##,OutletDHWTank_Connection_Type##OTHER##,OutletDHWTank_Connection_Size##OTHER##,OutletBoiler_Connection_Type##OTHER##,OutletBoiler_Connection_Size##OTHER##,OutletBoiler_Height##LENGTH##MILLIMETERS,Operating_Heating_Temperature##OTHER##,NominalLength##OTHER##,NominalHeight##OTHER##,NominalDepth##OTHER##,NBSReference##OTHER##,NBSOfficeMasterTag##OTHER##,NBSObjectName##OTHER##,NBSNote##OTHER##,NBSDescription##OTHER##,Mounting##OTHER##,ModelReference##OTHER##,ModelNumber##OTHER##,Model##OTHER##,Maximum_Operating_Pressure##OTHER##,Maximum_Heating_Temperature##OTHER##,Material##OTHER##,Manufacturer_Website##OTHER##,Manufacturer##OTHER##,ManufactureName##OTHER##,Interlocks##OTHER##,Insulation Thickness##OTHER##,InstallationDate##OTHER##,InletHeatPump_Connection_Type##OTHER##,InletHeatPump_Connection_Size##OTHER##,InletHeatPump_Height##LENGTH##MILLIMETERS,InletHC_Connection_Type##OTHER##,InletHC_Connection_Size##OTHER##,InletHC_Height##LENGTH##MILLIMETERS,InletDHWTank_Connection_Type##OTHER##,InletDHWTank_Connection_Size##OTHER##,InletDHWTank2_Height##LENGTH##MILLIMETERS,InletDHWTank1_Height##LENGTH##MILLIMETERS,InletBoiler_Connection_Type##OTHER##,InletBoiler_Connection_Size##OTHER##,InletBoiler_Height##LENGTH##MILLIMETERS,Inlet/Outlet-HC/HeatPump/Boiler_ExternalDiameter##LENGTH##MILLIMETERS,Inlet/Outlet-HC/DHW/HeatPump_Offset##LENGTH##MILLIMETERS,Inlet/Outlet-DHWtankDiameter##LENGTH##MILLIMETERS,Inlet/Outlet-DHWTank_ExternalDiameter##LENGTH##MILLIMETERS,IfcExportType##OTHER##,IfcExportAs##OTHER##,IP_Rating##OTHER##,OutletDHWTank_Offset##LENGTH##MILLIMETERS,OutletHC_Offset##LENGTH##MILLIMETERS,TMU_Hight##LENGTH##MILLIMETERS,Gross_Weight##OTHER##,Fuse_Rating##OTHER##,Frequency##OTHER##,Finish##OTHER##,Features##OTHER##,External_Material##OTHER##,ExpectedLife##OTHER##,Energy_Efficiency_Class##OTHER##,DurationUnit##OTHER##,Diagonal_Size##OTHER##,Description##OTHER##,TMU_Depth##LENGTH##MILLIMETERS,CreatedOn##OTHER##,CreatedBy##OTHER##,Colour##OTHER##,Clerance zone visibility##OTHER##,ClearanceTop##LENGTH##MILLIMETERS,ClearanceLeft##LENGTH##MILLIMETERS,ClearanceFront##LENGTH##MILLIMETERS,ClearanceBottom##LENGTH##MILLIMETERS,ClearanceBack##LENGTH##MILLIMETERS,Clearance Right##LENGTH##MILLIMETERS,ClassifcationValue##OTHER##,ClassifcationName##OTHER##,CE_Approval##OTHER##,BarCode##OTHER##,BMS_Links##OTHER##,BIMObjectName##OTHER##,AssetType##OTHER##,AssetIdentifier##OTHER##,OutletHC/DHW_Height##LENGTH##MILLIMETERS,Inlet/Outlet-HC/HeatPump/BoilerDiameter##LENGTH##MILLIMETERS
TMU 500,,0,www.myaic.eu,0,16,DaPr,880.000000000000,500 litres,,,info@myaic.eu,years,0,,230.000000000000,www.myaic.eu,,1,116 W,365 kg,Rectangular (Vertical),0,n/a,,TMU,TMU 500,https://myaic.eu/downloads,880.000000000000,1048.000000000000,2171.000000000000,Threaded,G 2"",443.000000000000,Threaded,G 2"",Threaded,G 1 1/2"",Threaded,G 2"",1483.000000000000,35-85 C,880,1048,1233,87-97-12,n/a,AIC_StratifiedBufferTank,,n/a,Floor standing,TMU,TMU 500,TMU 500,6 bar,95 C,Steel,www.myaic.eu,AIC Europe BV,AIC Europe BV,Yes,60 mm Neodul light + 20mm fleece,,Threaded,G 2"",1293.000000000000,Threaded,G 2"",803.000000000000,Threaded,G 1 1/2"",1068.000000000000,1608.000000000000,Threaded,G 2"",1743.000000000000,50.000000000000,439.000000000000,54.700000000000,65.000000000000,Pset_TankTypeCommon,IfcTankType,X4D,564.000000000000,315.000000000000,2171.000000000000,803,6.3 A,50 Hz,Painted,,Steel,,C,years,650 (810),Thermal Management Unit is a stratification buffer tank combined with the heart of the system – a hybrid heat controller. Hybrid heat controller manages both heat sources; heat pump; and boiler; to deliver heat in the most efficient and cheapest way for the customer. Besides heat source control; the unit manages also up to 4 mixed circuits and Domestic Hot Water.,1022.000000000000,,DaPr,Telegrey,1,400.000000000000,100.000000000000,740.000000000000,0.000000000000,500.000000000000,100.000000000000,Pr_60_50_96,Uniclass2015,Yes,,Yes,AIC_StratifiedBufferTank_TMU_500-800,Fixed,n/a,2060.000000000000,44.300000000000
TMU 800,,0,www.myaic.eu,0,16,DaPr,990.000000000000,800 litres,,,info@myaic.eu,years,0,,230.000000000000,www.myaic.eu,,1,130 W,395 kg,Rectangular (Vertical),0,n/a,,TMU,TMU 800,https://myaic.eu/downloads,990.000000000000,1192.000000000000,2171.000000000000,Threaded,G 2 1/2"",443.000000000000,Threaded,G 2 1/2"",Threaded,G 1 1/2"",Threaded,G 2 1/2"",1483.000000000000,35-85 C,990,1048,1233,87-97-12,n/a,AIC_StratifiedBufferTank,,n/a,Floor standing,TMU,TMU 800,TMU 800,6 bar,95 C,Steel,www.myaic.eu,AIC Europe BV,AIC Europe BV,Yes,60 mm Neodul light + 20mm fleece,,Threaded,G 2 1/2"",1293.000000000000,Threaded,G 2 1/2"",803.000000000000,Threaded,G 1 1/2"",1068.000000000000,1608.000000000000,Threaded,G 2 1/2"",1743.000000000000,50.000000000000,495.000000000000,72.100000000000,80.000000000000,Pset_TankTypeCommon,IfcTankType,X4D,620.000000000000,370.000000000000,2171.000000000000,885,6.3 A,50 Hz,Painted,,Steel,,C,years,790 (950),Thermal Management Unit is a stratification buffer tank combined with the heart of the system – a hybrid heat controller. Hybrid heat controller manages both heat sources; heat pump; and boiler; to deliver heat in the most efficient and cheapest way for the customer. Besides heat source control; the unit manages also up to 4 mixed circuits and Domestic Hot Water.,1162.000000000000,,DaPr,Telegrey,1,400.000000000000,100.000000000000,740.000000000000,0.000000000000,500.000000000000,100.000000000000,Pr_60_50_96,Uniclass2015,Yes,,Yes,AIC_StratifiedBufferTank_TMU_500-800,Fixed,n/a,2060.000000000000,44.300000000000
